|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | |
| **rate LIST OF MATERIAL MANUFACTURING**  **BY**  **BUILDING CENTRE JAMMU**  **Sector 7, Lower Roop Nagar, Phase-1st, Jammu. Tel. /Fax: 0191 – 2592422, E – Mail: bcjjk93@rediffmail.com** | | | | | | | | | |
| **Sr.No** | **Name of the item** | **Area/Tile** | **coverage/sft** | | | | **GRAY** | **RED** | **YELLOW** |
| 1. **C.C.Tiles 1" THICK in ratio 1:2:4** | | | | | | | | | |
|  | 12”X12” | 1.00 sft | 1.00/sft | | | 16.50/= | | 18.00/= | 19.50/= |
|  | 14”X14” | 1.36 sft | 0.74/sft. | | | 19.50/= | | 21.00/= | 23.50/= |
|  | 10”X10” | 0.70 sft | 1.43/sft. | | | 11.75/= | | 12.75/= | 13.75/= |
| 1. **P. C. C TILES 2" THICK** | | | | |  | | | | |
|  | 12"X12" | 1.00 sft | 1.00/sft | | | **Ratio** | | | |
| **1:2:4** | | **1:3:6** | **1:4:8** |
| 26.50/= | | 21.50/= | 19.00/= |
| 1. **C.C.PAVERS 60 MM THICK in ratio 1:2:4** | | | | | | | | | |
|  | I-Shape Paver | 0.31 sft | 3.25/sft. | | | 10.50/= | | 11.00/= | 12.00/= |
|  | 10"x10" Grass Paver | 0.70 sft | 1.43/sft | | | 18.00/= | | 19.00/= | 20.00/= |
| 1. **R.c.c. slabs (hand made)** | | | | | | | | **1:2:4**  **(M-15)** | **ratio 1:1½:3**  **(M-20)** |
|  | 4’X1’X4½” | | | | | | | 850/= | 1000/= |
|  | 3’X1’X4½” | | | | | | | 675/= | 710/= |
|  | 2’X1’X4½” | | | | | | | 425/= | 450/= |
|  | 4’X1’X3” | | | | | | | 460/= | 485/= |
|  | 3’X1’X3” | | | | | | | 360/= | 380/= |
|  | 2’X1’X3” | | | | | | | 250/= | 270/= |
|  | 1’-6”X1’-6”X3” | | | | | | | 230/= | 250/= |
| 1. **c.c.blocks (sakar vibrating machine made)** | | | | | | | | **Ratio** | |
|  | 6”x7½"x11½" Plain | | | | | | | (1:4:8) | 29.00/= |
|  | 6”x7½"x11½" Plain | | | | | | | (1:5:10) | 25.50/= |
|  | 6”x7½"x11½" Plain | | | | | | | (1:6:12) | 23.50/= |
|  | 4”x7½"x11½" (Plain) | | | | | | | (1:4:8) | 20.50/= |
|  | 4”x7½"x11½" (Plain) | | | | | | | (1:5:10) | 18.50/= |
|  | 12”x8”x6” Hollow Blocks | | | | | | | (1:5:10) | 27.00/= |
|  | 12”x8”x6” Hollow Blocks | | | | | | | (1:4:8) | 30.00/= |
|  | 12”x8”x6” Hollow Blocks | | | | | | | (1:3:6) | 35.00/= |
| 1. **c.c. Drains hand made in ratio 1:2:4** | | | | | | | | | |
|  | 6” Drain size 1’-6” long | | | | | | | | 120.00/= |
|  | 9” Drain 2'-0" Long | | | | | | | | 190.00/= |
| 1. **c.c. bricks in (sakar machine made)** | | | | | | | | **Ratio1:5:10**  **(M-05)** | **ratio 1:4:8**  **(m-7.5)** |
|  | 9”x4¼"x2¾” Plain (Sakar/Vibrating Table) | | | | | | | 6.50/= | 7.00/= |
|  | 9”x4¼"x2¾” Colored Side | | | | | | | 8.00/= | 8.50/= |
|  | 9”x4¼"x2¾” Colored Top | | | | | | | 10.50/= | 11.00/= |
|  | 9”x4¼"x2¾” Colored L shape | | | | | | | 11.25/= | 11.75/= |
|  | 9”x4¼"x2¾” Colored U shape | | | | | | | 11.50/= | 12.00/= |
| 1. **c.c. hand made kerb stone ( ratio 1:2:4)** | | | | | | | |  | |
|  | 20"x12" x 6"+3" (Rounded)  2 | | | | | | | | 120.00/= |
| 1. **c.c. hydrolac machine kerb stone** | | | | **ratio** | | | | | |
| **1:1½:3** | | | | **1:2:4** | **1:4:8** |
|  | 12"x12" x 4"+2"  2 | | | 52.00/= | | | | 46.00/= | 33.00/= |
| **NOTE:**   1. Some of the items are readily available whereas some items may require some delivery time as we manufacture these items on order with advance payments. 2. The rates are exclusive of taxes, carriage, loading & unloading would be charged extra on actual basis. 3. Our products are qualitative, cost effective & competitive than market.   **For Building Centre Jammu**    **Sd/-**  **Authorized Signatory**  **No: BCJ/2016/ 171-76 Dated: 15.07.2016** | | | | | | | | | |